General

General

[image: ]General
SURVEY SELF-ASSESSMENT
ROTARY SCREW COMPRESSOR


	SECTION A – DETAILS (to be fully completed by SIP Sales)



	SIP SALES ORDER REF
	

	DISTRIBUTOR ACC NO.
	

	CUSTOMER NAME
	

	CUSTOMER ADDRESS
	

	MODEL
	

	DATE OF PURCHASE
	



	
IMPORTANT

· Screw compressors need to be used daily. It is essential that they pump (or make air) for a minimum of 1000 hours annually. This is 20 hours a week or 4 hours daily, for example. This is the minimum hours of producing air, not the hours the compressor is switched on.
· Failure to meet this requirement will severely damage the air end (pump) and can cause motor related issues.
· Not meeting the minimum air requirement will invalidate warranty.

If you are unsure about the suitability of this type of air compressor, please contact SIP Customer Service on 01509 500400 before completing your order. Alternatively, you can contact your local SIP dealer to discuss your air requirements.



	SECTION B – ELECTRICAL SUPPLY REQUIREMENT (tick one option below)

	1
	SINGLE PHASE
	2.2kW screw compressors require a 240v 16A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	2
	SINGLE PHASE
	3kW/4kW screw compressors require a 240v 32A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	3
	SINGLE PHASE
	5.5kW screw compressors require a 240v 32A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	4
	THREE PHASE
	4kW/5.5kW screw compressors require a 400v 20A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	5
	THREE PHASE
	7.5kW screw compressors require a 400v 32A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	6
	THREE PHASE
	11kW/15kW screw compressors require a 400v 40A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	7
	THREE PHASE
	22kW screw compressors require a 400v 63A fused supply with D-type MCBs
	☐ YES     ☐ N/A

	
· All electrical work should be undertaken by a qualified electrician.
· Mains supply isolator is recommended on installation.
· Models fitted with a dryer require an additional 230v supply.

By ticking the box, you agree that this will be the minimum supply you provide. All current National Electrical Installation standards should be adhered to. For cable sizes refer to the instruction manual.

The use of Phase Converters or Inverters is not recommended to any other none Standard Mains Electricity configurations, all of which are not covered by SIP Warranty term and conditions.






	LOCATION DETAILS
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ROOM

The dimensions of the space for the screw compressor shown are only indicative, but is advisable to follow them as closely as possible.

Access to the rear of the compressor is required for servicing. 50cm is the minimum access required while 100cm is preferable.

CONDENSATE MANAGEMENT

The Hazardous Waste regulations of 2005 affect all owners of compressed air systems with respect to the proper disposal of condensate.

The UK Water Resources Act states it is an offence to knowingly permit toxic waste entry to surface water or groundwater, with fines of £20,000 or more. Please ensure that Oil / Water Separators are used and that you comply with national and local legislation. Contact your local authority for help and advice.


	SECTION C – ENVIRONMENTAL FACTORS



· The area must be free of airborne contaminates, e.g. dust, abrasive particles, moisture or gases.
· The area of installation must be adequately protected from the environment.
· The area of installation must be well ventilated.
· Ensure that temperature of the working environment ranges between +2°C and 45°C. Compressor working temperature shall range between 75°C to 85°C (20°C to 25°C room temperature).

	ADDITIONAL NOTES



· Screw compressor air ends (pump) need to be ran for a minimum of 80 hours per month or 1000 hours annually.
· Should the screw compressor not be used for a month or more, please contact SIP Customer Service for advice.
· Pipework installations, filter equipment and all other ancillary equipment is the responsibility of the user. No consequential action will be accepted by SIP under any circumstances.
· Any compressor site in an unsafe area of access, e.g. in roof space, will not be serviced, maintained, repaired or warranted until moved to a safe working environment.
· You will need to provide a forklift truck or similar upon delivery of the compressor.
· The compressor is covered by a SIP 2-Year Standard Silver Warranty. The compressor must be registered online within 30 days and must have a paid service after the first year to quality or the second year.
· The paid service must be undertaken by SIP or an SIP Authorised Distributor.


	IMPORTANT

· By signing this survey you confirm that the distributor has discussed the suitability of the generator with you, including air consumption assessments, location, electrical installation and environmental conditions.
· You agree the compressor will pump (load) for a minimum of 20 hours per week and accept that failure to do so will invalidate warranty.
· You also agree to comply with the Environmental Factors as stated in Section C.
· A mis-sold or mis-purchased product is not covered by SIP T&Cs. If in doubt, contact SIP Customer Service or your distributor.



	END USER

	SIGNATURE
	

	PRINTED NAME
	

	DATE OF SIGNING
	



	SIP DISTRIBUTOR (please countersign below)

	SIGNATURE
	

	PRINTED NAME
	

	DATE OF SIGNING
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